[bookmark: _GoBack]Fully Y cable for information about RPM from ignition.
You must not use this Y cable. Relay will working with out information about RPM – non functional blocking of relay during running engine
Version with electronic switch inside of ignition.
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